**Universal Features**

**Manufactured to the exact size of your opening within 1/8 of an inch (3mm)**

* Assures door seals properly thereby improving insulating values and reducing noise and particle transfer between environments.
* Enhances appearance by not having unsightly gaps between the door panels or the frame.
* Eliminates the need for mismatched panel sizes or oversized/undersized seals to compensate for “standard” door sizes filling non-standard openings.

**Full perimeter air seals are standard on all full thickness models**

* Allows for the maximum environmental separation between areas thereby minimizing transfer of:
- Temperature
- Humidity
- Noise
- Dust
- Microbes

**Factory aligned hardware**

* Doors are centered correctly at the factory so you don’t need to in the field.
* Reduces installation time
* Assures proper field alignment

**Largest selection of hardware choices in the industry**

* Assorted Café style hinges for lighter duty options.
* Variety of spring assist features to ensure positive closure in wind load applications.

**Full height Mount Assembly on most full thickness models**

* Reinforces the panel strength from top to bottom by equally distributing the stress of impacts on the panel facing.
* Significantly reduces the cracking of door facings diagonally from the hardware that is common with competitive doors

**Dozens of optional features to match the needs of any environment**

* Window options in over a dozen size and design configurations and infinite custom configurations
* Locking accessories
* Closing assist options
* Washdown & USDA packages
* Wide array of Impact Protection features (Bumpers, Impact Panels, Kick Plates, Rub Rails, Jamb Guards)